Verifikation von Auslegungsverfahren für Hochleistungs-Schneckenförderer

Prof. Dr.-Ing. W. A. Günthner,
Dipl.-Ing. N. Blomeyer
Lehrstuhl für Fördertechnik Materialfluss Logistik, Technische Universität München 

Es werden Auslegungsverfahren für vertikale und horizontale bis leicht geneigte Hochleistungs-Schneckenförderer vorgestellt, die eine anwendbare und praxistaugliche Möglichkeit sind, solche Fördergeräte für den täglichen Einsatz im Massengutumschlag auszulegen. Die Verifikation des Auslegungsverfahrens für vertikale Schneckenförderer durch Leistungsmessungen an zwei Referenzanlagen hat gezeigt, dass sich die im industriellen Einsatz befindlichen Anlagen mit guten Ergebnissen durch das Berechnungsverfahren nachrechnen lassen.
This paper presents feasible and realistic designs for the daily use of vertical, horizontal and slightly tilted high-capacity screw conveyors in mass good transshipment. The design of vertical screw conveyors was verified by means of performance measurings at two industrial reference plants and the calculations showed good results.